{
"sdd_tacoma_tire_R": {
    "information":{
        "authors":"BeamNG",
        "name":"BFGoodrich K02 38x12.50R17 Rear Tires",
        "value":900,
    },
    "slotType" : "tire_R_trx",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["sdd_tacoma_tire", ["wheel_RR","tire_RR"], [], {"pos":{"x":-0.56, "y":0.0, "z":0.0}, "rot":{"x":0, "y":0, "z":180}, "scale":{"x":1.0, "y":1, "z":1}}],
        ["sdd_tacoma_tire", ["wheel_RL","tire_RL"], [], {"pos":{"x": 0.56, "y":0.0, "z":0.0}, "rot":{"x":0, "y":0, "z":0},   "scale":{"x":1.0, "y":1, "z":1}}],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$tirepressure_R", "range", "psi", "Wheels", 30, 0, 40, "Tire Pressure", "Relative to atmospheric pressure", {"subCategory":"Rear"}],
    ],
    "pressureWheels": [
        ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
        {"disableMeshBreaking":false,"disableHubMeshBreaking":false},
        {"hasTire":true},
        {"enableTireReinfBeams":false},
        {"enableTireLbeams":true},
        {"enableTireSideReinfBeams":true},
        {"enableTreadReinfBeams":true},
        {"enableTirePeripheryReinfBeams":true},

        //general settings
        {"radius":0.42},
        {"tireWidth":0.295},

        //tire options
        {"wheelSideBeamSpring":"$=$tirepressure_R*900","wheelSideBeamDamp":60},
        {"wheelSideBeamSpringExpansion":601000,"wheelSideBeamDampExpansion":40},
        {"wheelSideTransitionZone":0.1,"wheelSideBeamPrecompression":0.99},

        {"wheelSideReinfBeamSpring":"$=$tirepressure_R*300","wheelSideReinfBeamDamp":80},
        {"wheelSideReinfBeamSpringExpansion":201000,"wheelSideReinfBeamDampExpansion":40},
        {"wheelSideReinfTransitionZone":0.09,"wheelSideReinfBeamPrecompression":0.99},

        {"wheelReinfBeamSpring":4000,"wheelReinfBeamDamp":400},
        {"wheelReinfBeamDampCutoffHz":250,"wheelReinfBeamPrecompression":0.99},

        {"wheelTreadBeamSpring":61000,"wheelTreadBeamDamp":250},
        {"wheelTreadBeamDampCutoffHz":500,"wheelTreadBeamPrecompression":0.99},

        {"wheelTreadReinfBeamSpring":121000,"wheelTreadReinfBeamDamp":125},
        {"wheelTreadReinfBeamDampCutoffHz":500,"wheelTreadReinfBeamPrecompression":0.99},

        {"wheelPeripheryBeamSpring":41000,"wheelPeripheryBeamDamp":240},
        {"wheelPeripheryBeamDampCutoffHz":500,"wheelPeripheryBeamPrecompression":0.99},

        {"wheelPeripheryReinfBeamSpring":81000,"wheelPeripheryReinfBeamDamp":120},
        {"wheelPeripheryReinfBeamDampCutoffHz":500,"wheelPeripheryReinfBeamPrecompression":0.99},

        //general tire values
        {"nodeWeight":0.35},
        {"nodeMaterial":"|NM_RUBBER"},
        {"pressurePSI":"$tirepressure_R"},
        {"dragCoef":15},

        //groundmodel friction multipliers
        {"frictionCoef":1.0},
        {"slidingFrictionCoef":1.04},
        {"stribeckExponent":1.5},
        {"treadCoef":0.9},

        //advanced friction values
        {"noLoadCoef":1.4},
        {"loadSensitivitySlope":0.0001},
        {"fullLoadCoef":0.4},
        {"softnessCoef":0.9},

        //deform values
        {"wheelSideBeamDeform":37000,"wheelSideBeamStrength":44000},
        {"wheelTreadBeamDeform":29000,"wheelTreadBeamStrength":35000},
        {"wheelPeripheryBeamDeform":85000,"wheelPeripheryBeamStrength":85000},
    ],
},

}